|  |  |  |  |
| --- | --- | --- | --- |
| **Part Number Comparison Sheet** | | |  |
|  |  |  |  |
| **Fossil/Aquarian Original Part Number** | **Yarway Part Number** | **Product Description:  Fossil/Aquarian High Integrity Brazed Joint Probes:** | **Drawing Ref:** |
| 9300-0002 | 964584-01 | Aquarian High Pressure Probe for applications over 650psi | S822-605X |
| 9300-0010 | 964584-43 | Aquarian Low Pressure Probe for applications under 650psi | S912-613X |
| 9300-0010 | 964584-52 | Aquarian Low Pressure Probe for applications under 650psi | S912-613X |
| 9300-0006 |  | Aquarian Probe Fits Clark Reliance FG 3000PSI |  |
| 9300-0007 |  | Aquarian Probe Fits Clark Reliance ZG 2000PSI |  |
| 9300-0015 |  | Aquarian Probe Fits Clark Reliance Model V 1000PSI |  |
| 9300-013 |  | Aquarian Probe Fits Clark Reliance Model T 450 PSI |  |
| 9300-0016 |  | Aquarian Probe Fits Gilco 3/8" NPT 1800PSI |  |
| 9300-0017 |  | Aquarian Probe Fits Gilco 3/8" NPT 850PSI |  |
|  |  | **Fossil/Aquarian Modules & Replacement Mother Boards:** |  |
| 9310-9352 | 964584-02 | Aq 3000Classic Power Supply Module | S852-202X |
| 9310-9350 | 964584-03 | Aq 3000Classic D&V Module | S852-204X |
| 9310-9513 | 964584-04 | Aq 3000Classic System Monitor PCB Loaded | S852-203X |
| 9310-9510 | 964584-11 | Aq 3000Classic 10 Probe Mother Board | S852-201-10X |
| 9310-9510 | 964584-18 | Aq 3000Classic 10-12Probe Mother Board (N12/N4) | S852-201X |
| 9310-9511 | 964584-A1 | Aq 3000Classic 10-12P Mother Brd Loaded N4X | S852- 201.N4X |
| 9310-9361 | 966111-\*\* | Aq 3000Classic 4-20mA Module |  |
| 9320-0001 | 968652-01 | Aq 3000Mini Maintenance Kit |  |
| 9310-9600 | 968652-02 | Aq 3000Mini Module | S892-201X |
| 9310-9600 | 968652-05 | Aq 3000 Mini PCB Loaded 120V W/O Continuity | S892-201CX |
| 9310-9210 | 970198-09 | Aq 1000 Plus ElectronicsPCB 120V Form C | S895-201X |
| 9300-2300 | 971205-01 | Aq 120V Alarm Module & Relay Socket | S916-200X |
| 9310-9361 | 972349-17 | Aq 3000Classic 4-20module for 972-013 & 014 |  |
| 9300-2004 | 972349-18 | Aq 1000 Plus 4 Probe Junction Box |  |
|  |  | **Fossil/Aquarian Replacement Parts** |  |
| 9940-0202 | 104779-01 | Port Cover for Yarway Color Port |  |
| 9940-0202 | 112925 | Port Cover for Yarway Color Port |  |
| 1020-0002 | 16781 | Belleville Washer S/S Spring Cone for Bi Color Gage" " |  |
| 1000-0030 | 954181-09 | Cap Screw (Flange Bolt) 3/8-16 x 1 3/8" " |  |
| 1020-0400 | 917211-01 | Washer for Bi Color Gage |  |
| 9320-0100 | 918159-01 | Ported Guage Kit to fit Yarway Ported Gauge |  |
| 1080-0018 | 919051 | Retaining Spring for Bi Color Gage |  |
| 9320-0100 | 923321 | Bi-Color Ported Gage Kit |  |
| 1170-0302 | 964584019 | Swagelok Plug SS-810P |  |
|  |  | LED Illuminator to Fit Yarway Ported Gauges |  |
|  |  | LED Illuminator To Fit Flat Glass Gauges |  |
| 1500-0632 |  | Gasket for \* aftermarket Probes |  |
| 9900-7140 |  | Vertical Extension Rod for Probes 3.5" each addition inch |  |
|  |  |  |  |
| **Original Fossil Parts and Equipment are only available in the UK from Fire Protection Centre** | | | |